

#           _   _               ___     ______  _   _
#          | \ | | ___  _ __ __| \ \   / /  _ \| \ | |
#          |  \| |/ _ \| '__/ _` |\ \ / /| |_) |  \| |
#          | |\  | (_) | | | (_| | \ V / |  __/| |\  |
#          |_| \_|\___/|_|  \__,_|  \_/  |_|   |_| \_|
#


client
dev tun
proto udp
remote 191.101.1.212 1194
resolv-retry infinite
nobind
tun-mtu 1500
tun-mtu-extra 32
mssfix 1450
persist-key
persist-tun
ping 15
ping-restart 0
ping-timer-rem
reneg-sec 0

remote-cert-tls server

#mute 10000
# Read authentication persisted from env
auth-user-pass /config/openvpn-credentials.txt

comp-lzo
verb 3
pull
fast-io
cipher AES-256-CBC

<ca>
-----BEGIN CERTIFICATE-----
MIID2jCCA0OgAwIBAgIJAMgRqbAv02GFMA0GCSqGSIb3DQEBBQUAMIGlMQswCQYD
VQQGEwJVUzELMAkGA1UECBMCQ0ExFTATBgNVBAcTDFNhbkZyYW5jaXNjbzEVMBMG
A1UEChMMRm9ydC1GdW5zdG9uMRIwEAYDVQQLFAl2cG4tdXNfdjExEjAQBgNVBAMU
CXZwbi11c192MTESMBAGA1UEKRQJdnBuLXVzX3YxMR8wHQYJKoZIhvcNAQkBFhBp
bmZvQG5vcmR2cG4uY29tMB4XDTE0MDUyMDA2MDQxNVoXDTI0MDUxNzA2MDQxNVow
gaUxCzAJBgNVBAYTAlVTMQswCQYDVQQIEwJDQTEVMBMGA1UEBxMMU2FuRnJhbmNp
c2NvMRUwEwYDVQQKEwxGb3J0LUZ1bnN0b24xEjAQBgNVBAsUCXZwbi11c192MTES
MBAGA1UEAxQJdnBuLXVzX3YxMRIwEAYDVQQpFAl2cG4tdXNfdjExHzAdBgkqhkiG
9w0BCQEWEGluZm9Abm9yZHZwbi5jb20wgZ8wDQYJKoZIhvcNAQEBBQADgY0AMIGJ
AoGBANEl+rFOCVuwJ9z2Wa1l3VHCZd4TIvk2sHbWblAcO5rHl4CzmDu9MFJ+/A+h
032qlS6Ths8OzgkVW7q0zCMcbq23uU7hjtnJff6dtzUZ0X5gYlHRFWpiRk1APx3C
7paU6hd+yrcTaTnmY0Xn+7bx0wZTa3zQN6EUjvTJwe9OkLu1AgMBAAGjggEOMIIB
CjAdBgNVHQ4EFgQULjoVWQtYVrs372OjrGzwxFGPFVUwgdoGA1UdIwSB0jCBz4AU
LjoVWQtYVrs372OjrGzwxFGPFVWhgaukgagwgaUxCzAJBgNVBAYTAlVTMQswCQYD
VQQIEwJDQTEVMBMGA1UEBxMMU2FuRnJhbmNpc2NvMRUwEwYDVQQKEwxGb3J0LUZ1
bnN0b24xEjAQBgNVBAsUCXZwbi11c192MTESMBAGA1UEAxQJdnBuLXVzX3YxMRIw
EAYDVQQpFAl2cG4tdXNfdjExHzAdBgkqhkiG9w0BCQEWEGluZm9Abm9yZHZwbi5j
b22CCQDIEamwL9NhhTAMBgNVHRMEBTADAQH/MA0GCSqGSIb3DQEBBQUAA4GBALrm
IBxtJCqOrYkBh5F9cSP6SHWxWHpuLixtGl0rc1N8n/XHFFew+ade/SQrBorZFyHy
/KnvBEp6bnoTy/VLKPS/Hk2CpstDKp5JJHjyn/mdpjLKjvsnGDuOOCx0d5DQ+uFg
0pe8QtP86QYBeChjGiiOsB3t/oPGGS3fJiIsMJfe
-----END CERTIFICATE-----
</ca>
key-direction 1
<tls-auth>
#
# 2048 bit OpenVPN static key
#
-----BEGIN OpenVPN Static key V1-----
4217afe20847ddae049667566f18f685
f5428d1ba6b4d8d7070ee5c1ca97c7ca
d2161e1f37c1ee286c313f3044f9702d
137d65b548cb03714286b9169fc48a2e
2348626afb4b56e07f368c5e607b3846
c332b192c57b60a0964b8e5e38b9af9e
f8b5292376787de485209156ff0808b0
4e22feab670e7dd58b668427aca1c04b
84ef915de5fc687b0406be81e0a0aacd
11011c8b28fdfb541f3ea574b9996b10
fc86972da60ee7dedcec5585b9443777
7984400f2df06f1a57ce10b4137336f5
30aec6e1287d71edd78f9b8afe75c44d
2a4060fd46cb228dd467118caa8a5c67
e78180039da609c766174aba038b5b37
253fb3806f75d6318d72dbc6333a3228
-----END OpenVPN Static key V1-----
</tls-auth>

# OpenVPN controls startup and shut down of transmission
script-security 2
up /etc/transmission/start.sh
down /etc/transmission/stop.sh

