

#           _   _               ___     ______  _   _
#          | \ | | ___  _ __ __| \ \   / /  _ \| \ | |
#          |  \| |/ _ \| '__/ _` |\ \ / /| |_) |  \| |
#          | |\  | (_) | | | (_| | \ V / |  __/| |\  |
#          |_| \_|\___/|_|  \__,_|  \_/  |_|   |_| \_|
#


client
dev tun
proto tcp
remote 95.143.198.80 443
resolv-retry infinite
remote-random
nobind
tun-mtu 1500
tun-mtu-extra 32
mssfix 1450
persist-key
persist-tun
ping 15
ping-restart 0
ping-timer-rem
reneg-sec 0

remote-cert-tls server

#mute 10000
# Read authentication persisted from env
auth-user-pass /config/openvpn-credentials.txt

comp-lzo
verb 3
pull
fast-io
cipher AES-256-CBC

<ca>
-----BEGIN CERTIFICATE-----
MIID7DCCA1WgAwIBAgIJAOjT+K3VHk+hMA0GCSqGSIb3DQEBBQUAMIGrMQswCQYD
VQQGEwJTRTELMAkGA1UECBMCU0UxFTATBgNVBAcTDFNhbkZyYW5jaXNjbzEQMA4G
A1UEChMHTm9yZFZQTjELMAkGA1UECxMCU0UxGzAZBgNVBAMTEnRvci1zZS5ub3Jk
dnBuLmNvbTEbMBkGA1UEKRMSdG9yLXNlLm5vcmR2cG4uY29tMR8wHQYJKoZIhvcN
AQkBFhBtYWlsQGhvc3QuZG9tYWluMB4XDTE0MDQxNjEwMDU0N1oXDTI0MDQxMzEw
MDU0N1owgasxCzAJBgNVBAYTAlNFMQswCQYDVQQIEwJTRTEVMBMGA1UEBxMMU2Fu
RnJhbmNpc2NvMRAwDgYDVQQKEwdOb3JkVlBOMQswCQYDVQQLEwJTRTEbMBkGA1UE
AxMSdG9yLXNlLm5vcmR2cG4uY29tMRswGQYDVQQpExJ0b3Itc2Uubm9yZHZwbi5j
b20xHzAdBgkqhkiG9w0BCQEWEG1haWxAaG9zdC5kb21haW4wgZ8wDQYJKoZIhvcN
AQEBBQADgY0AMIGJAoGBAMJSO5D1v1ILhPNE3BY5ICnKluLGrPrKfJTxiQIUnPCe
Bdfy+m8Q4jNEuw4KAQyRkW1qxgcnNB/z9AbrkmKtEgiRKZbrSwqI48R1WKiRzqFW
KRz4StfAJ/ofI+fmW+kmaUUan/qmgTVFATA8hC/tE3iyjP1CiGXUMIFw31QULBKJ
AgMBAAGjggEUMIIBEDAdBgNVHQ4EFgQUICzd0OTOgTRgzoAq9Hv3nknHTYAwgeAG
A1UdIwSB2DCB1YAUICzd0OTOgTRgzoAq9Hv3nknHTYChgbGkga4wgasxCzAJBgNV
BAYTAlNFMQswCQYDVQQIEwJTRTEVMBMGA1UEBxMMU2FuRnJhbmNpc2NvMRAwDgYD
VQQKEwdOb3JkVlBOMQswCQYDVQQLEwJTRTEbMBkGA1UEAxMSdG9yLXNlLm5vcmR2
cG4uY29tMRswGQYDVQQpExJ0b3Itc2Uubm9yZHZwbi5jb20xHzAdBgkqhkiG9w0B
CQEWEG1haWxAaG9zdC5kb21haW6CCQDo0/it1R5PoTAMBgNVHRMEBTADAQH/MA0G
CSqGSIb3DQEBBQUAA4GBABeNfQHgAxIV4EDicSHSsKT84vfw+0+LGr/jsLo+XBJ9
kyCJR4VBVqt0WiBB5caqpv7tuU6XaTW5AvAMB8Edc1+8NfQFkpnaeGx8csR9iNwe
uOEMyrFCyFoovI/RefPXOJYkDwYXg8H/N0lHxR9NyrnK/vBg6g+TPp6S2C2Eknlf
-----END CERTIFICATE-----
</ca>
key-direction 1
<tls-auth>
#
# 2048 bit OpenVPN static key
#
-----BEGIN OpenVPN Static key V1-----
e1d3dd160e819f8661188d33b1f98238
8611c869c0138dab8dca6df3136376c3
d393787824a6b433c0da9762ecbbc41f
1d90b51ff30154fab74d07797f5136fb
825dfd331d30e140db73128d0f552e35
b11fc6e543f5f6e21a06e0278e8f604e
2666bb8c6396cc6c7d7f902c7a8f7498
41d17225cc4785f2ba6d9e81b73565a3
609ac7445ade1744c3e3be02d1d5eb9d
70b56be2918adf27f18714fbcb69821c
fb79d9cecb19b13de328684ab1ba95e1
754e9830535e9bc55f4295d133d0d332
bceb3cc0e6182847d6b5df6f645a656a
f6013e1147bf756ca4bdaad02a3929df
5c4037e035d143ab3effacab05cffe40
2e54a76bca1a99d0cda8d26fba31a2ff
-----END OpenVPN Static key V1-----
</tls-auth>

# OpenVPN controls startup and shut down of transmission
script-security 2
up /etc/transmission/start.sh
down /etc/transmission/stop.sh

