

#           _   _               ___     ______  _   _
#          | \ | | ___  _ __ __| \ \   / /  _ \| \ | |
#          |  \| |/ _ \| '__/ _` |\ \ / /| |_) |  \| |
#          | |\  | (_) | | | (_| | \ V / |  __/| |\  |
#          |_| \_|\___/|_|  \__,_|  \_/  |_|   |_| \_|
#


client
dev tun
proto udp
remote 192.99.168.52 1194
resolv-retry infinite
remote-random
nobind
tun-mtu 1500
tun-mtu-extra 32
mssfix 1450
persist-key
persist-tun
ping 15
ping-restart 45
ping-timer-rem
reneg-sec 0

remote-cert-tls server

#mute 10000
# Read authentication persisted from env
auth-user-pass /config/openvpn-credentials.txt

comp-lzo
verb 3
pull
fast-io
cipher AES-256-CBC

<ca>
-----BEGIN CERTIFICATE-----
MIIENzCCA6CgAwIBAgIJAJppFExlys5tMA0GCSqGSIb3DQEBBQUAMIHEMQswCQYD
VQQGEwJDQTERMA8GA1UECBMITW9udHJlYWwxETAPBgNVBAcTCE1vbnRyZWFsMR0w
GwYDVQQKExRhbnRpZGRvcy5ub3JkdnBuLmNvbTEdMBsGA1UECxMUYW50aWRkb3Mu
bm9yZHZwbi5jb20xHTAbBgNVBAMTFGFudGlkZG9zLm5vcmR2cG4uY29tMREwDwYD
VQQpEwhhbnRpZGRvczEfMB0GCSqGSIb3DQEJARYQaW5mb0Bub3JkdnBuLmNvbTAe
Fw0xNDA1MjExMTE4MDRaFw0yNDA1MTgxMTE4MDRaMIHEMQswCQYDVQQGEwJDQTER
MA8GA1UECBMITW9udHJlYWwxETAPBgNVBAcTCE1vbnRyZWFsMR0wGwYDVQQKExRh
bnRpZGRvcy5ub3JkdnBuLmNvbTEdMBsGA1UECxMUYW50aWRkb3Mubm9yZHZwbi5j
b20xHTAbBgNVBAMTFGFudGlkZG9zLm5vcmR2cG4uY29tMREwDwYDVQQpEwhhbnRp
ZGRvczEfMB0GCSqGSIb3DQEJARYQaW5mb0Bub3JkdnBuLmNvbTCBnzANBgkqhkiG
9w0BAQEFAAOBjQAwgYkCgYEA1G2T42fYUadGas6qPn8lfgl5NSbTpGsoScr8pK01
BtOgONwadJcgq0Hoy+a6/gyw2W/X4elRWhF054Uvaq+KLufezDOq2ltLKqpDtmOV
fr//jP79EwFf9Lu/DOfP+LwcrMh5LIwBk5WwgjuOZkFaCJE8Bn3qXNmQnFHmM+CQ
kKMCAwEAAaOCAS0wggEpMB0GA1UdDgQWBBS+SzJLvyuRe83shd5jIZB6HKXazDCB
+QYDVR0jBIHxMIHugBS+SzJLvyuRe83shd5jIZB6HKXazKGByqSBxzCBxDELMAkG
A1UEBhMCQ0ExETAPBgNVBAgTCE1vbnRyZWFsMREwDwYDVQQHEwhNb250cmVhbDEd
MBsGA1UEChMUYW50aWRkb3Mubm9yZHZwbi5jb20xHTAbBgNVBAsTFGFudGlkZG9z
Lm5vcmR2cG4uY29tMR0wGwYDVQQDExRhbnRpZGRvcy5ub3JkdnBuLmNvbTERMA8G
A1UEKRMIYW50aWRkb3MxHzAdBgkqhkiG9w0BCQEWEGluZm9Abm9yZHZwbi5jb22C
CQCaaRRMZcrObTAMBgNVHRMEBTADAQH/MA0GCSqGSIb3DQEBBQUAA4GBAMe+b+Wn
ZXjMoyWhSVXMR9+0zq65kc/IbuGegt4s+Y/xQqeFpvgBaTwnJth0y+A4o/jniSX/
Sde0+ibn96b208ADHhDbOAB2YKIBDPQp96LAsMJ/1uEK+8/NrhsZAn1lMDJBwfy0
xEmxoT4wALt5324FbvpBsAlkUpFc/laDfq36
-----END CERTIFICATE-----
</ca>
key-direction 1
<tls-auth>
#
# 2048 bit OpenVPN static key
#
-----BEGIN OpenVPN Static key V1-----
60bf45857b53a955318dcad691c4adb3
e3c64c381b4c31cade072d97e2c38faf
d9c4a87b4f4d3ec50baab8ca1a9e62ed
06fdf83cfea07b897a321208b990c4a1
010f1b803d98fe9c95d5de4a3e4254eb
1e1ccb9054db9baae5194d51ab09bc09
1837d12cace24bdc76edc3dd3ce5edae
3752f9699e37d68069bbc17d48f00c2f
d8dfceb07d830c421f77874774045b50
8c1f632e0337164adf5c678f434d7d38
123e9e865fa833d788d55faa09af9aa3
410d4bdea0b0d4550c89971bbaa66c08
f15aeb55483bccfd392212f15e4760f7
30160fffd368f28e6d0b6fb96a8198ee
79f6ea4f574151624fdbf513914e5295
ba35677fce8aeb8f09fb81c5ef697ff0
-----END OpenVPN Static key V1-----
</tls-auth>

# OpenVPN controls startup and shut down of transmission
script-security 2
up /etc/transmission/start.sh
down /etc/transmission/stop.sh

