

#           _   _               ___     ______  _   _
#          | \ | | ___  _ __ __| \ \   / /  _ \| \ | |
#          |  \| |/ _ \| '__/ _` |\ \ / /| |_) |  \| |
#          | |\  | (_) | | | (_| | \ V / |  __/| |\  |
#          |_| \_|\___/|_|  \__,_|  \_/  |_|   |_| \_|
#


client
dev tun
proto udp
remote 151.236.26.14 1194
resolv-retry infinite
remote-random
nobind
tun-mtu 1500
tun-mtu-extra 32
mssfix 1450
persist-key
persist-tun
ping 15
ping-restart 0
ping-timer-rem
reneg-sec 0

remote-cert-tls server

#mute 10000
# Read authentication persisted from env
auth-user-pass /config/openvpn-credentials.txt

comp-lzo
verb 3
pull
fast-io
cipher AES-256-CBC

<ca>
-----BEGIN CERTIFICATE-----
MIIDzjCCAzegAwIBAgIJAO2AmWYwWjCQMA0GCSqGSIb3DQEBBQUAMIGhMQswCQYD
VQQGEwJDSDELMAkGA1UECBMCQ0gxCzAJBgNVBAcTAk5BMRAwDgYDVQQKEwdOb3Jk
VlBOMQswCQYDVQQLEwJDSDEbMBkGA1UEAxMSdnBuLWNoLm5vcmR2cG4uY29tMRsw
GQYDVQQpExJ2cG4tY2gubm9yZHZwbi5jb20xHzAdBgkqhkiG9w0BCQEWEG1haWxA
aG9zdC5kb21haW4wHhcNMTQwNDE2MDgyNjAwWhcNMjQwNDEzMDgyNjAwWjCBoTEL
MAkGA1UEBhMCQ0gxCzAJBgNVBAgTAkNIMQswCQYDVQQHEwJOQTEQMA4GA1UEChMH
Tm9yZFZQTjELMAkGA1UECxMCQ0gxGzAZBgNVBAMTEnZwbi1jaC5ub3JkdnBuLmNv
bTEbMBkGA1UEKRMSdnBuLWNoLm5vcmR2cG4uY29tMR8wHQYJKoZIhvcNAQkBFhBt
YWlsQGhvc3QuZG9tYWluMIGfMA0GCSqGSIb3DQEBAQUAA4GNADCBiQKBgQCcyzh0
bY6WxemhW7hcvZpVJmOjcxZFCPyA7qeZs427czYpQmVc7M1xwSlsqK5GpHhR+Zg4
Fsa/1aXScN79qt5kIl3XCZJBuJA3jl9qL6uJ3FBL5SxENckWFd1XRF45OVDsLQLx
CLcif9mVKcQKgO+HR0YkP8sOLo2IgiN3t915LwIDAQABo4IBCjCCAQYwHQYDVR0O
BBYEFPs8M3RTCZzwuy19MJsQJcOeQ8P7MIHWBgNVHSMEgc4wgcuAFPs8M3RTCZzw
uy19MJsQJcOeQ8P7oYGnpIGkMIGhMQswCQYDVQQGEwJDSDELMAkGA1UECBMCQ0gx
CzAJBgNVBAcTAk5BMRAwDgYDVQQKEwdOb3JkVlBOMQswCQYDVQQLEwJDSDEbMBkG
A1UEAxMSdnBuLWNoLm5vcmR2cG4uY29tMRswGQYDVQQpExJ2cG4tY2gubm9yZHZw
bi5jb20xHzAdBgkqhkiG9w0BCQEWEG1haWxAaG9zdC5kb21haW6CCQDtgJlmMFow
kDAMBgNVHRMEBTADAQH/MA0GCSqGSIb3DQEBBQUAA4GBAHuQPBRHvot8KiT7BRN6
92eN1aiFjBo68ICyRVGWlHth2oz6to5XpsAgdpAnt36oeUGsfEA8eNnODW5HwBbB
Qpb99v7z0YUTZrxuEFL3DANR3UorR/+eTbFAYD5qi7eDAH+XWbaOoVdDJg500T4G
zySMCNLU6pv9z+qLq2+/cjZG
-----END CERTIFICATE-----
</ca>
key-direction 1
<tls-auth>
-----BEGIN OpenVPN Static key V1-----
358ece4e1ffbc48fc7a1908cba721292
2fad03d74e8c907ea6067974e2af7ff5
94bb8d0afdbf1c1debe28876fdb040d5
e92a23b3c9911042b5b6e424ea1d2d03
7acf31b82ec1f7f22123f35d3c89b685
f1b3ba4af07a78c093a861017e73f997
67108b42aa40af6a7b5bb5b41ad29a2f
ab5764a8e3e8299dfabf2372402b60a5
c7d63e4f65b4b5b77e4a4f92bc91863b
3293608e931183b8cdf1066df0b302fc
34052bed0a8b4d1b4bb4d39952ea397d
a31ac2d7313eb680c031058d50e2f167
e05832a4c1f94489963efc851c1329a2
37931460c7950ea49e6d763bc6070a63
3445d67fedb70f4b5ebcda5508f3d3ed
6c8702ec2ed2d690dba719ef3c3c88d6
-----END OpenVPN Static key V1-----
</tls-auth>
# OpenVPN controls startup and shut down of transmission
script-security 2
up /etc/transmission/start.sh
down /etc/transmission/stop.sh

